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UPCOMING MATCH #: _____________     BUMPER COLOR FOR MATCH (CIRCLE ONE):     RED      BLUE 

	IN PIT (ROBOT OFF) – NOTE REPAIRS

	❏ Change bumpers for upcoming match. Attached well?
❏ Plug in Driver Console laptop to charge.
❏ Check for loose parts/motors/gearboxes/wires/hoses
❏ Check battery cable connections to PDP & breaker
❏ Any dangling or damaged wires?
	❏ Check screws/connections on subsystems:
· DRIVETRAIN – Plates, motors, wheels
· INTAKE – Shafts, standoffs, brackets
· LAUNCHER/PLACER – Shafts, structure
· CLIMBER – Bolts, structure, shafts



	NON-POWERED SUBSYSTEM CHECKS – NOTE REPAIRS

	❏ DRIVETRAIN
	Rotation / Steering / Power transmission / Clean?

	❏ INTAKE

	Shaft collars tight / Belts tight and aligned / Structural alignment
Deployment moves correctly / Check motor and/or piston mounts

	❏ LAUNCHER/PLACER
	Structural alignment / Belts to motors properly attached / Wheels/rollers spin smoothly / Aiming system

	❏ CLIMBER
	Structure (wear or stress?) Hooks straight? / Strap wound properly, ratchet in correct position

	❏ ELECTRICAL
	Unmanaged or dangling wires / Check wires near moving or sharp parts for wear / CAN wire check / Components securely mounted

	❏ BUMPERS
	Correct color / Brackets intact and firm / Missing or loose hardware 



	IN PIT (ROBOT ON) - NOTE ANY CODE OR MECHANICAL CHANGES

	What changed?
	Notes:

	


	



	ENABLE ROBOT: POWERED SUBSYSTEM FUNCTIONAL CHECKS – NOTE REPAIRS

	❏ Electronic Components
	RSL: Blinking orange
Camera(s): Feed(s) working on dashboard
Radio: Securely mounted / Power and data cables / Connection


	❏ Drivetrain (wheels off the ground!)
	Drive wheels Forward / Back / Turning / Properly aligned?

	❏ Intake
	Deploy / Retract / Run intake / Run outtake / Reset for match

	❏ Launcher/Placer
	Loading / Run up to speed / check aiming

	❏ Climber
	Full extension / Retraction / Reset for match

	❏ Pneumatics: 
	Release Valve Closed / Holding Pressure / Watch gauge for leaks
Pressure:     ❏ 60psi working   ❏ 120psi stored



	ROBOT OFF (preparing to queue):

	❏ Install New Battery #_________________________
❏ Secure connector and Tug Test. Connector ok?
Battery Beak:
❏ Charge: ____________
❏ Status: _____________
	❏ Pack Driver Station with Laptop, controllers, charger
❏ Pack Robot Cart with necessary items: 
    ❏ Tools                            ❏ Team Flag
    ❏ Spare Battery              ❏ Gaffer’s Tape
    ❏ USB Tether Cable
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